Table of contents
TECE sanitary modules
TECE sanitary modules
TECEprofil toilet module with Octa II
cistern, 8 cm, installation height
1120 mm Toilet module including “easy
fit” flush plate installation. For
fitting to TECEprofil section tubes or
for installation in metal or wooden stud
walls and as a pre-wall or corner module
also suitable for single block assembly.
Octa II cistern 8 cm, for front
actuation:
- Safety tank made of impact-resistant
plastic, tested to EN 14055
- Cistern fully pre-assembled and sealed
- Cistern connection with outer thread R
1/2” at the top, compatible with quick
adapters
- 7-litre tank volume 6-litre pre-set
standard flush volume, 4.5-litre flush
volume can be set at any time 3-litre
partial flush volume for dual-flush
system optional setting of a 4/2 litre
flush volume possible.
- Insulated against condensation water
- For TECE flush plates and toilet flush
handle
- Can be used as a single or dual-flush
cistern
- “easy fit” flush plate installation
- Installation tunnel for service
opening, can be shortened without tools
- Low-noise hydraulic filling valve,
fitting group 1 according to DIN 4109
Module frame:
- Self-supporting, powder-coated
- Two M 12 retaining bolts and nuts
- Toilet drain bend DN 90/90 PE-HD,
including protective plug
- Toilet connection set DN 90
- Suitable for floor projections up to
30 cm
- Ceramics installation spacing 180 mm
or 230 mm
- Including wall attachment
Order No.: 9300500